Dear Sirs:

Many thanks for your enquiry! Please kindly check the below best quotation we offer to you. And don't hesitate to contact us if you have any questions, hoping to work as your partner in near future, you are welcome to visit us!

**PART 1 MAIN TECHNICAL INFORMATION**

|  |  |
| --- | --- |
| Diesel engine model | MAN 6L27/38 |
| Number of cylinders | 6 |
| Cylinder bore | 270mm |
| Piston stroke | 380mm |
| Rotate speed | 720rpm |
| Engine power | 1980kw |
| Generator set power | 1900kw |
| Generator type | HYUNDAI  HFJ7710-10P |
| HZ | 60hz |
| Voltage | 690v |
| POWER FACTOR （lag ） | 0.9 |
| Manufacturer | DOOSAN– MAN authorized manufacturer/ Korea |
| Year of made | 2020 |
| Dimensions | 7557\*3712\*2570mm |
| Weight （dry weight） | 44500kg |

**PART 2 SUPPLY LIST OF OTHER DOCUMENTS**

2.1 OPERATING INSTRUCTIONS

2.2 WORKING INSTRUCTIONS

2.3 FAT REPORT

**PART 3 SUPPLY SCOPE**

3.1 MAN 6L27//38 engine


3.2 HYUNDAI HFJ7710-10P generator

**PART 4 PICTURES AND DEMENSIONS**

****

****

****



**PART 6 QUOTATIONS**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **NAME** | **MODEL** | **Q'TY** | **Per/SET (USD)** | **TOTAL AMOUNT**  **(USD)** |
| 1 | GENERATOR SET | DOOSAN-MAN 6L27/38 1900 Kw x 720 RPM x 690v x 60 Hz | 4 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **REMARKS AND INSTRUCTIONS:** | | | |
| 1. PRICE TERMS : EXW WORKS QINHUANGDAO CHINA IN USD, OTHER CHARGES AT COST. EXCHANGE RATE IS SET 1USD≥7.07RMB. | | | |
| 2. VALIDITY : 60 DAYS, SUBJECT TO PRIOR SALE. |  |  |  |
| 3. CONDITION : MADE IN KOREA, JUST DID FOR TEST RUNNING, NOT PUT INTO COMMERCIAL OPERATION. | | | |
| 4. PAYMENT TERMS : BY T/T 30% IN ADVANCE, THE BALANCE PAID BEFORE SHIPMENT. | | |  |
| 5.DELIVERY TIME : IN STOCK, IMMEDIATELY DELIVERY AVALIABLE. | |  |  |